# Schaerer Coffee Soul 10 and 12 – configure to your needs

The Schaerer Coffee Soul is available in two versions and with three freely selectable user interfaces for different applications – it also has a wide range of modular accessories to choose from. Both machines can be optically configured. The Coffee Soul 10 features a 10.4-inch touch screen, the Coffee Soul 12 a high-resolution 12.1-inch video touch screen.

Technical data  
Recommended average daily output 250 cups

Mains connection 380 V – 415 V~, 50/60 Hz, 3L/N/PE

Fuse 3 x 16 A

Water infeed G3/8"

Input pressure 1 – 6 bar

Water drain ø 19 mm

Weight approx. 55 kg (net)

Continuous noise level ‹70 dB(A)

Dimensions  
Width 330 mm  
Height 732 mm  
Depth 576 mm

## Manufacturer Schaerer AG - <www.schaerer.com>

Performance description  
The machine is equipped with a grounds container that holds up to 550 grams (around 50 cups) and ensures that the entire coffee station stays clean. The clearly visible coloured cup positioning aid is clamped onto the cup tray for correct positioning with single and double outlets. This is particularly useful for self-service mode.

BestFoam  
The patented BestFoam technology gives the milk foam an incomparable quality. Choose from hot and cold milk foam as well as four different consistencies from firm to liquid.

Powder system  
Containers for chocolate and milk powder as well as other powder beverages are available in two versions:  
Individual container for one powder or Twin Topping container with separation for two different types of powder.

Additional bean hoppers and grinders  
Three bean hoppers for 1200 gram each can be installed. There is also the option of equipping the machine with grinders with special espresso grinding discs to achieve even higher beverage quality.

Second and third boiler  
Depending on the configuration, up to three stainless steel boilers can be installed. This makes it possible to dispense hot water, steam and coffee separately or simultaneously.

Additional water for americanos.   
The central outlet can be fitted with separate hot water dispensing for preparing the perfect americano.

Hot & Cold   
Cold beverages can be served in top quality with this feature: The coffee is brewed hot and then automatically cooled down to 30 to 35 degrees Celsius. This means that ice cubes do not melt as quickly and the intensity of flavour and aroma is retained.

Automatic or manually adjustable beverage outlet  
The outlet height can be set manually or automatically for each cup height.   
Heights between 65 and 185 millimetres are possible.

“Supersteam”, “Autosteam” and “Powersteam” steam wands  
There are three variants for heating and foaming milk:  
  
Variant 1 “Supersteam”The milk is heated and foamed fully automatically. The temperature and foaming can be programmed. The temperature and foaming can be programmed.

Variant 2“Autosteam”The milk is heated and foamed fully automatically. The temperature can be programmed.

Variant 3 “Powersteam”   
The milk is heated and foamed manually.

## Uptime! descaling system The Uptime! descaling system prevents malfunctions caused by limescale and the display reports when descaling is necessary. No technician is needed for the automatic descaling process.

**Cleaning**  
Cleaning takes place automatically through the display in line with the configured cleaning schedule.    
Cleaning programmes can be carried out manually at any time using the “Additional cleaning” function.

Schaerer Coffee Link: digital & smart  
Schaerer Coffee Link is a service platform that enables digital analyses and coffee machine control in real time.

Optional accessories  
We also offer the following additional optional accessories: Cup dispenser, under-counter cooling unit, cooling units and payment system.

## ProCare cleaning system ProCare is a programmable cleaning system that lasts for up to 100 autonomous cleaning cycles outside of ongoing operation.

Flavour Point syrup station  
The “Flavour Point” optional accessory is a syrup station that dispenses four different syrup flavours and is placed under the counter of the coffee machine. A flavour such as caramel or vanilla can be set in the beverage configuration.

„Cup & Cool  
“Cup & Cool” combines a cup warmer with a milk cooling unit, saving valuable space on the counter.   
The wide model holds 9.5 litres of milk, the narrow model 4 litres. The wide version can be perfectly positioned between two machines for central supply.

Side cooling unit  
The external cooling unit for the SOUL is available in black or with a stainless steel front, offering storage of up to 10 litres of fresh milk. To save space, the cooling unit is placed directly to the side of a machine or between two machines.

Twin side cooling unit  
The Schaerer cooling unit for two types of milk features two 4.5-litre milk containers for different types of milk. The Schaerer cooling unit with the “Twin Milk” variant is placed next to the machine or under the counter to save space.

Wide and narrow cup warmers  
The illuminated Schaerer cup warmers are available in wide and narrow versions and can be integrated perfectly into any counter concept. Thanks to their surfaces made of shatterproof glass and high-quality stainless steel, they are also easy to clean.

Lockable  
The front, cooling unit, bean hopper and powder container can be locked – ideal for self-service mode.

Installation  
Electricity, water and drainage for connecting lines must be connected by trained specialists.